### Summary

Design Name | main
Fitting Status | Successful
Software Version | H.42
Device Used | XC9572XL-7-TQ100
Date | 2- 7-2006, 10:44AM

##### RESOURCES SUMMARY

Macrocells Used | Pterms Used | Registers Used | Pins Used | Function Block Inputs Used
--- | --- | --- | --- | ---
66/72 (92%) | 228/360 (64%) | 30/72 (42%) | 55/72 (77%) | 130/216 (61%)

##### PIN RESOURCES

Signal Type | Required | Mapped
--- | --- | ---
Input | 6 | 6
Output | 24 | 24
Bidirectional | 24 | 24
GCK | 0 | 0
GTS | 0 | 0
GSR | 1 | 1
Pin Type | Used | Total
--- | --- | ---
I/O | 52 | 66
GCK/IO | 2 | 3
GTS/IO | 0 | 2
GSR/IO | 1 | 1

##### GLOBAL RESOURCES

Signal mapped onto global output enable net (GSR) | nRst

##### POWER DATA

Macrocells in high performance mode (MCHP) | 66
Macrocells in low power mode (MCLP) | 0
Total macrocells used (MC) | 66